6.0.3 Fast charge recognition page
Description
The top row of data from left to right are boot record time and onboard
temperature respectively;
The uppercase data on the left is voltage, current, and power from top to
bottom; The trigger time limit on the right is the setting menu -> trigger
-> trigger time value.Trigger timing is the timing of trigger time,When the
timing reaches the trigger time limit,The meter will stop triggering. Note
that:After some protocols stop triggering, the charger will restart.
The dark blue below the trigger timing is the load resistance.
The first column of the bottom white table is D+, D- voltage;The second
column is the current charging agreement that may be in progress;The third
column is the status bar.
当触发计时为启动时，显示为
,停止时为
; 当仪表未触发任何快
充协议时为
，已触发某种快充协议，如 QC2.0 时，为
.
Instructions
(1) Long press the left button: prompt to enter the fast charge trigger module, if a certain protocol
has been triggered, it will prompt to release.
(2) Click the middle button: start/stop the trigger timing.
(3) Long press the middle button: prompt to clear the trigger timing.
(4) Long press the right button: enter the charging tool menu (please see the subsequent
instructions).
13