9.0.3 Read DASH cable
Enter this function,Plug in the DASH cable,You
can read the chip-related data,As shown below
9.0.4 Analog DASH cable
This function is used without DASH cable
The USB-A head of the DASH cable will have one more data pin than the
ordinary USB-A data cable.And one more chip,Used to identify and start
VOOC/WARP flash charge.
If,The phone normally needs to use a USB-A->Type-C DASH cable,But
there is no such thread in hand,Only FNB48 tester and a C-C cable,But want
to trigger VOOC/WARP flash charge,At this time, the function of
simulating DASH cable can be started,And use the C-C cable to connect to
the phone, You can perform VOOC/WARP flash charging.
Note: Since this method does not use the original data cable for
charging, The charging power is largely affected by the C-C line,If the
impedance of the C
-C line is high,Then the charging power will be reduced a lot.
9.0.5 Apple 2.4A acceleration
When the Apple device detects that the charging head D+ and D- are
2.7V,To charge at 5V-2.4A,This function sets D+ and D- to 2.7V.
25