3.0 Performance description
3.0.1 Interface
1 Input monitoring port: USB-A, 9-PIN male;
2 Input monitoring port: TYPE-C, 24-PIN female seat;
3 Input monitoring port: Micro-USB, 5-PIN female socket; 4 output
monitoring ports: USB-A, 9-PIN female socket;
5 Output monitoring port: TYPE-C, 24-PIN female socket;
6 PC connection port: Micro-USB, 5-PIN female socket.
3.0.2 Human-computer interaction
1 1.77 inch TFT-LCD screen;
2
Multi-function switch;
3 Touch switch.
3.0.3 Voltage and Current
1The highest six-digit display of voltage, current and power, the highest
resolution is 0.00001 (V/A/W);
2 Record the minimum, maximum and average values of voltage, current,
and power during operation;
2 10 sets of switchable capacity, power, and time statistics;
3 1 set of voltage and current curve records, maximum support 9 hours
4 Support low-speed waveform (voltage, current, D+, D-) drawing, 2sps-
>100sps sampling rate;
5 Support high-speed ripple (voltage, AC coupling) drawing, up to 3.2Msps
sampling rate;
3.0.4 Fast charge trigger
1 QC2.0,QC3.0
;
trigger
2 Huawei FCP,SCP
;
trigger
3
Samsung AFC trigger;
5