Static Call Graph - [.\STM32F429_439xx\STM32F429_439xx.axf]

# Static Call Graph for image .\STM32F429_439xx\STM32F429_439xx.axf

#<CALLGRAPH># ARM Linker, 5.03 [Build 76]: Last Updated: Tue Aug 04 09:36:33 2015

### Maximum Stack Usage = 148 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ OV2640_Init ⇒ OV2640_DMA_Init ⇒ DMA_DeInit

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(i.BusFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DCMI_IRQHandler from stm32f4xx_it.o(i.DCMI_IRQHandler) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(i.HardFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(i.MemManage_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(i.NMI_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(i.PendSV_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - Reset_Handler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(i.SVC_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(i.SysTick_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(i.SystemInit) referenced from startup_stm32f429_439xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UsageFault_Handler from stm32f4xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f429_439xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429_439xx.o(.text)
  - fputc from usart.o(i.fputc) referenced from printf5.o(i.__0printf$5)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_uldivmod

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  DCMI_CaptureCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_CaptureCmd))
  [Called By]

  - >> main

  DCMI_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_ClearITPendingBit))
  [Called By]

  - >> DCMI_IRQHandler

  DCMI_Cmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_Cmd))
  [Called By]

  - >> main

  DCMI_GetITStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_GetITStatus))
  [Called By]

  - >> DCMI_IRQHandler

  DCMI_IRQHandler (Thumb, 26 bytes, Stack size 8 bytes, stm32f4xx_it.o(i.DCMI_IRQHandler))
  [Stack]

  - Max Depth = 8
  - Call Chain = DCMI_IRQHandler
  [Calls]
  - >> DCMI_GetITStatus
  - >> DCMI_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  DCMI_ITConfig (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_ITConfig))
  [Called By]

  - >> OV2640_DCMI_Config

  DCMI_Init (Thumb, 54 bytes, Stack size 12 bytes, stm32f4xx_dcmi.o(i.DCMI_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = DCMI_Init
  [Called By]
  - >> OV2640_DCMI_Config

  DCMI_JPEGCmd (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dcmi.o(i.DCMI_JPEGCmd))
  [Called By]

  - >> OV2640_DCMI_Config

  DCMI_OV2640_ReadID (Thumb, 84 bytes, Stack size 16 bytes, dcmi_ov2640.o(i.DCMI_OV2640_ReadID))
  [Stack]

  - Max Depth = 56
  - Call Chain = DCMI_OV2640_ReadID ⇒ DCMI_SingleRandomRead
  [Calls]
  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead
  [Called By]
  - >> main

  DCMI_SingleRandomRead (Thumb, 294 bytes, Stack size 40 bytes, sccb.o(i.DCMI_SingleRandomRead))
  [Stack]

  - Max Depth = 40
  - Call Chain = DCMI_SingleRandomRead
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_ReceiveData
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> DCMI_OV2640_ReadID

  DCMI_SingleRandomWrite (Thumb, 160 bytes, Stack size 32 bytes, sccb.o(i.DCMI_SingleRandomWrite))
  [Stack]

  - Max Depth = 32
  - Call Chain = DCMI_SingleRandomWrite
  [Calls]
  - >> I2C_SendData
  - >> I2C_Send7bitAddress
  - >> I2C_GenerateSTOP
  - >> I2C_GenerateSTART
  - >> I2C_CheckEvent
  [Called By]
  - >> SCCB_WriteRegs
  - >> OV2640_Reset
  - >> OV2640_JPEGConfig
  - >> OV2640_BrightnessConfig
  - >> DCMI_OV2640_ReadID

  DMA_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dma.o(i.DMA_Cmd))
  [Called By]

  - >> main

  DMA_DeInit (Thumb, 272 bytes, Stack size 28 bytes, stm32f4xx_dma.o(i.DMA_DeInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = DMA_DeInit
  [Called By]
  - >> OV2640_DMA_Init

  DMA_Init (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_dma.o(i.DMA_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_Init
  [Called By]
  - >> OV2640_DMA_Init

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  Delay (Thumb, 16 bytes, Stack size 8 bytes, main.o(i.Delay))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay
  [Called By]
  - >> main

  GPIO_Init (Thumb, 162 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> SCCB_GPIO_Config
  - >> OV2640_DCMI_Config
  - >> MCO1_Init
  - >> STM_EVAL_COMInit
  - >> main

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(i.GPIO_PinAFConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> SCCB_GPIO_Config
  - >> OV2640_DCMI_Config
  - >> MCO1_Init
  - >> STM_EVAL_COMInit

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> main

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  I2C_AcknowledgeConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_AcknowledgeConfig))
  [Called By]

  - >> SCCB_GPIO_Config
  - >> DCMI_SingleRandomRead

  I2C_CheckEvent (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_CheckEvent))
  [Called By]

  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead

  I2C_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_Cmd))
  [Called By]

  - >> SCCB_GPIO_Config

  I2C_DeInit (Thumb, 56 bytes, Stack size 8 bytes, stm32f4xx_i2c.o(i.I2C_DeInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = I2C_DeInit
  [Calls]
  - >> RCC_APB1PeriphResetCmd
  [Called By]
  - >> SCCB_GPIO_Config

  I2C_GenerateSTART (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_GenerateSTART))
  [Called By]

  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead

  I2C_GenerateSTOP (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_GenerateSTOP))
  [Called By]

  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead

  I2C_Init (Thumb, 172 bytes, Stack size 32 bytes, stm32f4xx_i2c.o(i.I2C_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> SCCB_GPIO_Config

  I2C_ReceiveData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_ReceiveData))
  [Called By]

  - >> DCMI_SingleRandomRead

  I2C_Send7bitAddress (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_Send7bitAddress))
  [Called By]

  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead

  I2C_SendData (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_i2c.o(i.I2C_SendData))
  [Called By]

  - >> DCMI_SingleRandomWrite
  - >> DCMI_SingleRandomRead

  MCO1_Init (Thumb, 72 bytes, Stack size 16 bytes, dcmi_ov2640.o(i.MCO1_Init))
  [Stack]

  - Max Depth = 36
  - Call Chain = MCO1_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_MCO1Config
  - >> RCC_ClockSecuritySystemCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> OV2640_Init

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  NVIC_Init (Thumb, 92 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> OV2640_DMA_Init
  - >> OV2640_DCMI_Config

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> OV2640_DMA_Init
  - >> OV2640_DCMI_Config

  OV2640_AutoExposure (Thumb, 44 bytes, Stack size 0 bytes, dcmi_ov2640.o(i.OV2640_AutoExposure))
  [Stack]

  - Max Depth = 40
  - Call Chain = OV2640_AutoExposure ⇒ SCCB_WriteRegs ⇒ DCMI_SingleRandomWrite
  [Calls]
  - >> SCCB_WriteRegs
  [Called By]
  - >> main

  OV2640_BrightnessConfig (Thumb, 56 bytes, Stack size 8 bytes, dcmi_ov2640.o(i.OV2640_BrightnessConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = OV2640_BrightnessConfig ⇒ DCMI_SingleRandomWrite
  [Calls]
  - >> DCMI_SingleRandomWrite
  [Called By]
  - >> main

  OV2640_DCMI_Config (Thumb, 346 bytes, Stack size 64 bytes, dcmi_ov2640.o(i.OV2640_DCMI_Config))
  [Stack]

  - Max Depth = 84
  - Call Chain = OV2640_DCMI_Config ⇒ GPIO_Init
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> DCMI_JPEGCmd
  - >> DCMI_Init
  - >> DCMI_ITConfig
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_AHB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> OV2640_Init

  OV2640_DMA_Init (Thumb, 124 bytes, Stack size 80 bytes, dcmi_ov2640.o(i.OV2640_DMA_Init))
  [Stack]

  - Max Depth = 108
  - Call Chain = OV2640_DMA_Init ⇒ DMA_DeInit
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> RCC_AHB1PeriphClockCmd
  - >> DMA_Init
  - >> DMA_DeInit
  [Called By]
  - >> OV2640_Init

  OV2640_Init (Thumb, 34 bytes, Stack size 8 bytes, dcmi_ov2640.o(i.OV2640_Init))
  [Stack]

  - Max Depth = 116
  - Call Chain = OV2640_Init ⇒ OV2640_DMA_Init ⇒ DMA_DeInit
  [Calls]
  - >> SCCB_GPIO_Config
  - >> OV2640_Reset
  - >> OV2640_DMA_Init
  - >> OV2640_DCMI_Config
  - >> MCO1_Init
  - >> Delay_ms
  [Called By]
  - >> main

  OV2640_JPEGConfig (Thumb, 300 bytes, Stack size 16 bytes, dcmi_ov2640.o(i.OV2640_JPEGConfig))
  [Stack]

  - Max Depth = 56
  - Call Chain = OV2640_JPEGConfig ⇒ OV2640_Reset ⇒ DCMI_SingleRandomWrite
  [Calls]
  - >> DCMI_SingleRandomWrite
  - >> OV2640_Reset
  - >> Delay_ms
  [Called By]
  - >> main

  OV2640_Reset (Thumb, 22 bytes, Stack size 8 bytes, dcmi_ov2640.o(i.OV2640_Reset))
  [Stack]

  - Max Depth = 40
  - Call Chain = OV2640_Reset ⇒ DCMI_SingleRandomWrite
  [Calls]
  - >> DCMI_SingleRandomWrite
  [Called By]
  - >> OV2640_JPEGConfig
  - >> OV2640_Init

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_AHB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB1PeriphClockCmd))
  [Called By]

  - >> SCCB_GPIO_Config
  - >> OV2640_DMA_Init
  - >> OV2640_DCMI_Config
  - >> MCO1_Init
  - >> STM_EVAL_COMInit

  RCC_AHB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_AHB2PeriphClockCmd))
  [Called By]

  - >> OV2640_DCMI_Config

  RCC_APB1PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> SCCB_GPIO_Config
  - >> STM_EVAL_COMInit
  - >> main

  RCC_APB1PeriphResetCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB1PeriphResetCmd))
  [Called By]

  - >> I2C_DeInit

  RCC_APB2PeriphClockCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> STM_EVAL_COMInit

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_ClockSecuritySystemCmd))
  [Called By]

  - >> MCO1_Init

  RCC_GetClocksFreq (Thumb, 132 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 16
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init
  - >> I2C_Init
  - >> main

  RCC_MCO1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(i.RCC_MCO1Config))
  [Called By]

  - >> MCO1_Init

  SCCB_GPIO_Config (Thumb, 150 bytes, Stack size 32 bytes, sccb.o(i.SCCB_GPIO_Config))
  [Stack]

  - Max Depth = 80
  - Call Chain = SCCB_GPIO_Config ⇒ I2C_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> I2C_Init
  - >> I2C_DeInit
  - >> I2C_Cmd
  - >> I2C_AcknowledgeConfig
  [Called By]
  - >> OV2640_Init

  SCCB_WriteRegs (Thumb, 26 bytes, Stack size 8 bytes, dcmi_ov2640.o(i.SCCB_WriteRegs))
  [Stack]

  - Max Depth = 40
  - Call Chain = SCCB_WriteRegs ⇒ DCMI_SingleRandomWrite
  [Calls]
  - >> DCMI_SingleRandomWrite
  [Called By]
  - >> OV2640_AutoExposure

  STM_EVAL_COMInit (Thumb, 204 bytes, Stack size 32 bytes, stm324x9i_eval.o(i.STM_EVAL_COMInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> USART_Config

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(i.SystemInit))
  [Stack]

  - Max Depth = 24
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(.text)

  TimingDelay_Decrement (Thumb, 16 bytes, Stack size 0 bytes, main.o(i.TimingDelay_Decrement))
  [Called By]

  - >> SysTick_Handler

  USART_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_Cmd))
  [Called By]

  - >> STM_EVAL_COMInit

  USART_Config (Thumb, 42 bytes, Stack size 24 bytes, usart.o(i.USART_Config))
  [Stack]

  - Max Depth = 104
  - Call Chain = USART_Config ⇒ STM_EVAL_COMInit ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> STM_EVAL_COMInit
  [Called By]
  - >> main

  USART_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> fputc
  - >> USART_Transmit

  USART_Init (Thumb, 174 bytes, Stack size 32 bytes, stm32f4xx_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 48
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> STM_EVAL_COMInit

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_usart.o(i.USART_SendData))
  [Called By]

  - >> fputc
  - >> USART_Transmit

  USART_Transmit (Thumb, 30 bytes, Stack size 16 bytes, usart.o(i.USART_Transmit))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_Transmit
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> main

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  __0printf$5 (Thumb, 22 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf$5 (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printf5.o(i.__0printf$5))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> main

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 30 bytes, Stack size 16 bytes, usart.o(i.fputc))
  [Stack]

  - Max Depth = 16
  - Call Chain = fputc
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Address Reference Count : 1]
  - printf5.o(i.__0printf$5)

  main (Thumb, 410 bytes, Stack size 32 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 148
  - Call Chain = main ⇒ OV2640_Init ⇒ OV2640_DMA_Init ⇒ DMA_DeInit
  [Calls]
  - >> DCMI_Cmd
  - >> DCMI_CaptureCmd
  - >> GPIO_ReadInputDataBit
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_GetClocksFreq
  - >> DMA_Cmd
  - >> USART_Transmit
  - >> USART_Config
  - >> OV2640_JPEGConfig
  - >> OV2640_Init
  - >> OV2640_BrightnessConfig
  - >> OV2640_AutoExposure
  - >> DCMI_OV2640_ReadID
  - >> Delay
  - >> __2printf
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  ### Local Symbols

  SetSysClock (Thumb, 190 bytes, Stack size 16 bytes, system_stm32f4xx.o(i.SetSysClock))
  [Stack]

  - Max Depth = 16
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  Delay_ms (Thumb, 18 bytes, Stack size 0 bytes, dcmi_ov2640.o(i.Delay_ms))
  [Called By]

  - >> OV2640_JPEGConfig
  - >> OV2640_Init

  _printf_core (Thumb, 658 bytes, Stack size 104 bytes, printf5.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  [Called By]
  - >> __0printf$5

  ### Undefined Global Symbols