10.1.7 Current change wake up
Set the wake-up current,When the current change exceeds the wake-up
current,The meter changes from standby state to normal working
state,When set to 0, this function is turned off.
10.1.8 Bluetooth switch
After closing, Bluetooth data transmission is not possible
10.1.9 Gravity direction recognition
When opened,Automatically switch page orientation,After closing,Unable
to automatically switch the page reverse,But you can switch the page
direction by long pressing the middle button on the (6.0.1) simple page.
10.1.10 Boot page
Turn on/off the boot page.
10.1.11 Reset
Restore all settings except the recorded data
10.2 Settings menu -> Record
Set the configuration required for logging data.
10.2.1 Curve recording time
Set the recording time of the voltage and current curve,Maximum 9
hours,Set to no time record.Every time you change the configuration, the
curve will be cleared to 0.
10.2.2 Statistical current threshold
When the current ≥ the threshold,To carry out
statistics on capacity, energy, and time,Setting
range 0-5A.
10.2.3 Energy statistics time
Set to no time,No time limit,Until the statistics reach the maximum
value. After setting the time,When the statistical time reaches the
set value, the statistics will automatically stop.
10.2.7 Clear all records
Clear all recorded data,Including offline curves,Energy statistics.
10.3 Trigger related configuration
Trigger related configuration.
27