4.0 Structure appearance
1 Input monitoring port: USB-A, 9-PIN male;
2 Input monitoring port: TYPE-C, 24-PIN female socket;
3 input monitoring port: Micro-USB, 5-PIN female
socket; 4 output monitoring port: TYPE-C, 24-PIN
female socket; 5 PD communication switch
6 output monitoring port: USB-A, 9-PIN
female; 7 touch switch: BACK button;
8 Multi-function switches: left button, middle button, right
button; 9 PC connection port: Micro-USB, 5-PIN female socket..
7